{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":15,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Spectrum efficiency for Best Subcarrier achievable Rate based algorithm:"]
[]
[7.4255634572343903,7.3297234012689039,7.2346935952265836,7.1475277810824531,7.0816615458644057,7.0127674154285096,6.9466085740430472,6.8883528988502798,6.8374256880120194,6.7943849219062242,6.7445373383875653,6.7050459202753228,6.6656501797860574,6.6281615338661961,6.589998154897418]

{"sheet":"Sheet2","index":1,"n_rows":3,"n_cols":15,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Spectrum efficiency for Subcarrier achievable data-Rate based algorithm:"]
[]
[7.4481606083406566,7.4102408844754475,7.3714138580977098,7.3345484161710806,7.3129271976298709,7.2852630497992639,7.2577848685315169,7.2316694060592495,7.2106022133284293,7.1956670785556733,7.1673855777762512,7.1517364438351718,7.1372459277395874,7.116395122622472,7.0956768228566478]