{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":10,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Spectrum efficiency for best subcarrier CSI based algorithm:"]
[]
[5.7173128970681719E-3,1.7666961381366718E-2,5.5011278878915021E-2,0.16350607714904233,0.45050969107410227,1.06221452828136,2.0792458856672527,3.4315583552006519,4.9667979288345814,6.5910228859991165]

{"sheet":"Sheet2","index":1,"n_rows":3,"n_cols":10,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Spectrum efficiency for Subcarrier Achievable data-Rate based algorithm:"]
[]
[7.3418468213580484E-3,2.2591771821331361E-2,6.903981143671431E-2,0.19699599979699367,0.50236381489636805,1.1299299010275998,2.1796011083727986,3.5653737899598403,5.1132066531254647,6.7349606599775456]

{"sheet":"Sheet3","index":2,"n_rows":3,"n_cols":10,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Spectrum efficiency for Searching method:"]
[]
[7.4063763417289447E-3,2.2804393460672624E-2,6.9672686819786084E-2,0.19881026756610667,0.50613428254736736,1.1408741745276019,2.202580249154829,3.5973968328836246,5.15057099748784,6.7756469572177105]